#Notes 2880 dpi, uni-directional.
#PRINTER=Quad1400
# Original Curve by Lou Dina 7/26/2011

# Re-purposed for Chrome Metallic Luster photo paper

CURVE_NAME=1400CL-ChromeMetalLus-Selenium-ACV
GRAPH_CURVE=YES
N_OF_INKS=6
DEFAULT_INK_LIMIT=
BOOST_K=25
LIMIT_K=15
LIMIT_C=6
LIMIT_M=6
LIMIT_Y=0
LIMIT_LC=0
LIMIT_LM=0

# This section determines the shape of the black ink curve
N_OF_GRAY_PARTS=1
GRAY_INK_1=K
GRAY_VAL_1=100
GRAY_HIGHLIGHT=4
GRAY_SHADOW=4
GRAY_OVERLAP=
GRAY_GAMMA=1.5
GRAY_CURVE=

# If toner inks are used (I'm not using them with the Claria inkset) you would use this section. 


# Toner Partition Information

N_OF_TONER_PARTS=0
TONER_INK_1=
TONER_VAL_1=
TONER_INK_2=
TONER_VAL_2=

TONER_HIGHLIGHT=10
TONER_SHADOW=10
TONER_GAMMA=2
TONER_CURVE=

# N_OF_TONER_2_PARTS=0
# TONER_2_HIGHLIGHT=10
# TONER_2_SHADOW=10
# TONER_2_GAMMA=1
# TONER_2_CURVE=

N_OF_UNUSED=
UNUSED_INK_1=
UNUSED_INK_2=
UNUSED_INK_3=
UNUSED_INK_4=
UNUSED_INK_5=

# The following are manually defined curve shapes for the colored curves
# You can change curves by changing the X/Y coordinates
#  Below curve is Roy's tone-curve.acv, but I have lowered the maximum ink from 94 to 20 at 80K for finer control

CURVE_C="0;0 15;2.5 40;9 62;17 80;20 88;17 94;10.6 100;0"
COPY_CURVE_M=C
COPY_CURVE_Y=C
COPY_CURVE_LC=C
COPY_CURVE_LM=C
LINEARIZE="86.74 84.62 82.25 79.43 76.42 73.44 69.9 66.14 62.13 58.3 53.81 49.43 44.36 39 34.22 28.93 23.14 18.09 13.85 5.82 3.11"
