 #Notes 2880 dpi, uni-directional.
#PRINTER=Quad1400
# Curve by Lou Dina 7/24/2011


CURVE_NAME=1400CL-CrPortRag-VeryWarm
GRAPH_CURVE=YES
N_OF_INKS=6
DEFAULT_INK_LIMIT=100
BOOST_K=
LIMIT_K=45
LIMIT_C=0
LIMIT_M=0
LIMIT_Y=18
LIMIT_LC=0
LIMIT_LM=22

N_OF_GRAY_PARTS=1
GRAY_INK_1=K
GRAY_VAL_1=100
GRAY_HIGHLIGHT=10
GRAY_SHADOW=12
GRAY_OVERLAP=
GRAY_GAMMA=2.0
GRAY_CURVE=

#
# Toner Partition Information
#
N_OF_TONER_PARTS=0
TONER_INK_1=
TONER_VAL_1=
TONER_INK_2=
TONER_VAL_2=

TONER_HIGHLIGHT=10
TONER_SHADOW=10
TONER_GAMMA=1
TONER_CURVE=


N_OF_TONER_2_PARTS=0
TONER_2_HIGHLIGHT=10
TONER_2_SHADOW=10
TONER_2_GAMMA=1
TONER_2_CURVE=

N_OF_UNUSED=
UNUSED_INK_1=
UNUSED_INK_2=
UNUSED_INK_3=
UNUSED_INK_4=
UNUSED_INK_5=

CURVE_C="0;0 10;0 20;0 30;0 40;2 50;8 60;13 70;15 80;14 90;10 100;0"
CURVE_Y="0;0 10;1 20;2 30;5 40;10 50;15 60;18 70;20 80;19 90;14 100;0"
COPY_CURVE_M=C
COPY_CURVE_LC=Y
COPY_CURVE_LM=Y
LINEARIZE="98 94.45 89.95 84.42 78.18 72.11 65.33 59.18 53.66 49.31 44.83 40.84 37.18 33.71 31.21 28.88 26.06 23.6 21.63 18.78 16.67"
