#Notes 2880 dpi, uni-directional.
#PRINTER=Quad1400
# Curve by Lou Dina 7/21/2011

# Red River Polar Matte. 

CURVE_NAME=1400CL-RRPM-Neutral-ACV
GRAPH_CURVE=YES
N_OF_INKS=6
DEFAULT_INK_LIMIT=100
BOOST_K=50
LIMIT_K=30
LIMIT_C=0
LIMIT_M=2
LIMIT_Y=0
LIMIT_LC=0
LIMIT_LM=0

# This section determines the shape of the black ink curve
N_OF_GRAY_PARTS=1
GRAY_INK_1=K
GRAY_VAL_1=100
GRAY_HIGHLIGHT=10
GRAY_SHADOW=12
GRAY_OVERLAP=
GRAY_GAMMA=1
GRAY_CURVE=

# If toner inks are used (they aren't with the Claria inkset) you would use this section. 
# I have made this section inactive. If using toners, activate by removing the pound signs

# Toner Partition Information
#
N_OF_TONER_PARTS=0
TONER_INK_1=
TONER_VAL_1=
TONER_INK_2=
TONER_VAL_2=

TONER_HIGHLIGHT=10
TONER_SHADOW=10
TONER_GAMMA=2
TONER_CURVE=

# N_OF_TONER_2_PARTS=0
# TONER_2_HIGHLIGHT=10
# TONER_2_SHADOW=10
# TONER_2_GAMMA=1
# TONER_2_CURVE=

N_OF_UNUSED=
UNUSED_INK_1=
UNUSED_INK_2=
UNUSED_INK_3=
UNUSED_INK_4=
UNUSED_INK_5=

# The following are manually defined curve shapes for the colored curves
# You can change curves by changing the X/Y coordinates
#  Below curve is Roy's tone-curve.acv, but I have lowered the maximum ink from 94 to 20 at 80K for finer control

CURVE_C="0;0 15;2.5 40;9.3 62;17 80;20 88;17 94;10.6 100;0"
COPY_CURVE_M=C
COPY_CURVE_Y=C
COPY_CURVE_LC=C
COPY_CURVE_LM=C
LINEARIZE="95.73 93.05 89.47 84.72 79.49 74.13 68.13 62.41 56.8 51.69 46.19 41.39 37.24 33.75 30.39 26.91 23.24 20.01 17.87 15.19 12.92"
