#Notes 2880 dpi, uni-directional.
#PRINTER=Quad1400
# Curve by Lou Dina 7/21/2011

# RR Polar Matte

CURVE_NAME=1400CL-RRPM-WARM-ACV
GRAPH_CURVE=YES
N_OF_INKS=6
DEFAULT_INK_LIMIT=100
BOOST_K=50
LIMIT_K=26
LIMIT_C=0
LIMIT_M=12
LIMIT_Y=15
LIMIT_LC=0
LIMIT_LM=0

# This section determines the shape of the black ink curve
N_OF_GRAY_PARTS=1
GRAY_INK_1=K
GRAY_VAL_1=100
GRAY_HIGHLIGHT=10
GRAY_SHADOW=12
GRAY_OVERLAP=
GRAY_GAMMA=1
GRAY_CURVE=

# If toner inks are used (they aren't with the Claria inkset) you would use this section. 
# I have made this section inactive. If using toners, activate by removing the pound signs

# Toner Partition Information
#
N_OF_TONER_PARTS=0
TONER_INK_1=
TONER_VAL_1=
TONER_INK_2=
TONER_VAL_2=

TONER_HIGHLIGHT=10
TONER_SHADOW=10
TONER_GAMMA=2
TONER_CURVE=

# N_OF_TONER_2_PARTS=0
# TONER_2_HIGHLIGHT=10
# TONER_2_SHADOW=10
# TONER_2_GAMMA=1
# TONER_2_CURVE=

N_OF_UNUSED=
UNUSED_INK_1=
UNUSED_INK_2=
UNUSED_INK_3=
UNUSED_INK_4=
UNUSED_INK_5=

# The following are manually defined curve shapes for the colored curves
# You can change curves by changing the X/Y coordinates
#  Below curve is Roy's tone-curve.acv, but I have lowered the maximum ink from 94 to 20 at 80K for finer control

CURVE_C="0;0 15;2.5 40;9.3 62;17 80;20 88;17 94;10.6 100;0"
COPY_CURVE_M=C
COPY_CURVE_Y=C
COPY_CURVE_LC=C
COPY_CURVE_LM=C
LINEARIZE="95.8 92.69 88.89 84.07 78.66 73.36 67.39 61.53 55.96 51.07 45.51 40.84 36.08 32.15 29.47 26.15 23 20.14 17.88 15 13.12"
