#Notes 2880 dpi, uni-directional.
#PRINTER=Quad1400
# Curve by Lou Dina 7/21/2011
# Red River Premium Matte Paper - alpha cellulose bright white matte paper

# This first section sets ink limits for each ink

CURVE_NAME=1400CL-RRPrMatPlus-Neutral
GRAPH_CURVE=YES
N_OF_INKS=6
DEFAULT_INK_LIMIT=100
BOOST_K=50
LIMIT_K=40
LIMIT_C=0
LIMIT_M=0
LIMIT_Y=1
LIMIT_LC=0
LIMIT_LM=5

# This section determines the shape of the black ink curve
N_OF_GRAY_PARTS=1
GRAY_INK_1=K
GRAY_VAL_1=100
GRAY_HIGHLIGHT=4
GRAY_SHADOW=8
GRAY_OVERLAP=
GRAY_GAMMA=2.2
GRAY_CURVE=

# If toner inks are used (they aren't with the Claria inkset) you would use this section. 
# I have made this section inactive. If using toners, activate by removing the pound signs

# Toner Partition Information
#
# N_OF_TONER_PARTS=0
# TONER_INK_1=
# TONER_VAL_1=
# TONER_INK_2=
# TONER_VAL_2=

# TONER_HIGHLIGHT=10
# TONER_SHADOW=10
# TONER_GAMMA=1
# TONER_CURVE=

# N_OF_TONER_2_PARTS=0
# TONER_2_HIGHLIGHT=10
# TONER_2_SHADOW=10
# TONER_2_GAMMA=1
# TONER_2_CURVE=

N_OF_UNUSED=
UNUSED_INK_1=
UNUSED_INK_2=
UNUSED_INK_3=
UNUSED_INK_4=
UNUSED_INK_5=

# The following are manually defined curve shapes for the colored curves
# You can change curves by changing the X/Y coordinates

CURVE_C="0;0 10;0 20;0 30;0 40;2 50;8 60;13 70;15 80;13 90;7 100;0"
COPY_CURVE_M=C
CURVE_Y="0;0 10;1 20;2 30;5 40;10 50;15 60;19 70;20 80;17 90;7 100;0"
COPY_CURVE_LC=Y
COPY_CURVE_LM=Y
LINEARIZE="96.35 93.14 89.47 85 80.09 75.42 69.86 64.48 59.38 54.49 49.24 43.86 38.44 33.93 30.44 27.34 23.64 20.25 17.77 15.34 13.89"


