 #Notes 2880 dpi, uni-directional.
#PRINTER=Quad1400
# Curve by Lou Dina 7/16/2011


CURVE_NAME=1400CL-CrPortRag-Neutral2
GRAPH_CURVE=YES
N_OF_INKS=6
DEFAULT_INK_LIMIT=100
BOOST_K=
LIMIT_K=45
LIMIT_C=0
LIMIT_M=0
LIMIT_Y=2
LIMIT_LC=0
LIMIT_LM=10

N_OF_GRAY_PARTS=1
GRAY_INK_1=K
GRAY_VAL_1=100
GRAY_HIGHLIGHT=10
GRAY_SHADOW=12
GRAY_OVERLAP=
GRAY_GAMMA=2
GRAY_CURVE=

#
# Toner Partition Information
#
N_OF_TONER_PARTS=0
TONER_INK_1=
TONER_VAL_1=
TONER_INK_2=
TONER_VAL_2=

TONER_HIGHLIGHT=10
TONER_SHADOW=10
TONER_GAMMA=1
TONER_CURVE=


N_OF_TONER_2_PARTS=0
TONER_2_HIGHLIGHT=10
TONER_2_SHADOW=10
TONER_2_GAMMA=1
TONER_2_CURVE=

N_OF_UNUSED=
UNUSED_INK_1=
UNUSED_INK_2=
UNUSED_INK_3=
UNUSED_INK_4=
UNUSED_INK_5=

CURVE_C="0;0 10;0 20;0 30;0 40;2 50;8 60;13 70;15 80;13 90;7 100;0"
COPY_CURVE_M=C
CURVE_Y="0;0 10;1 20;2 30;5 40;10 50;16 60;21 70;23 80;19 90;7 100;0"
COPY_CURVE_LC=Y
COPY_CURVE_LM=Y
LINEARIZE="97.98 94.82 90.68 85.26 79.29 73.46 67.1 60.98 55.42 50.96 46.33 42.1 38.28 34.81 32.42 30.04 27.11 24.6 22.37 19.04 16.85"