#Notes 2880 dpi, uni-directional.
#PRINTER=Quad1400
# Original Curve by Lou Dina 7/26/2011

# Chrome Metallic Luster photo paper

CURVE_NAME=1400CL-ChromeMetalLus-Neutral-ACV
GRAPH_CURVE=YES
N_OF_INKS=6
DEFAULT_INK_LIMIT=100
BOOST_K=25
LIMIT_K=17
LIMIT_C=0
LIMIT_M=0
LIMIT_Y=0
LIMIT_LC=0
LIMIT_LM=0

# This section determines the shape of the black ink curve
N_OF_GRAY_PARTS=1
GRAY_INK_1=K
GRAY_VAL_1=100
GRAY_HIGHLIGHT=4
GRAY_SHADOW=4
GRAY_OVERLAP=
GRAY_GAMMA=1.5
GRAY_CURVE=

# If toner inks are used (I'm not using them with the Claria inkset) you would use this section. 


# Toner Partition Information

N_OF_TONER_PARTS=0
TONER_INK_1=
TONER_VAL_1=
TONER_INK_2=
TONER_VAL_2=

TONER_HIGHLIGHT=10
TONER_SHADOW=10
TONER_GAMMA=2
TONER_CURVE=

# N_OF_TONER_2_PARTS=0
# TONER_2_HIGHLIGHT=10
# TONER_2_SHADOW=10
# TONER_2_GAMMA=1
# TONER_2_CURVE=

N_OF_UNUSED=
UNUSED_INK_1=
UNUSED_INK_2=
UNUSED_INK_3=
UNUSED_INK_4=
UNUSED_INK_5=

# The following are manually defined curve shapes for the colored curves
# You can change curves by changing the X/Y coordinates
#  Below curve is Roy's tone-curve.acv, but I have lowered the maximum ink from 94 to 20 at 80K for finer control

CURVE_C="0;0 15;2.5 40;9 62;17 80;20 88;17 94;10.6 100;0"
COPY_CURVE_M=C
COPY_CURVE_Y=C
COPY_CURVE_LC=C
COPY_CURVE_LM=C
LINEARIZE="88.913809 87.127222 84.708157 82.633072 79.848194 77.273997 74.012496 70.645952 67.051383 63.506658 59.222682 55.275944 50.085462 44.610438 39.446771 33.175951 26.955724 21.279246 16.841804 7.147681 3.464335"
